void setup()

{

pinMode(10, OUTPUT);

pinMode(9, OUTPUT);

pinMode(8, OUTPUT);

}

void loop()

{

digitalWrite(10, HIGH); // For green LED

delay(2000); // Wait for 2 second

digitalWrite(10, LOW);

digitalWrite(9, HIGH); // For orange LED

delay(3000); // Wait for 3 second

digitalWrite(9, LOW);

digitalWrite(8, HIGH); // For the red LED

delay(2000); // Wait for 2 second

digitalWrite(8, LOW);

}







